Pipe data SOR

Pipe data

All pipe data required to calculate the noise emission is summarized on this entry page. During the calculation of the valve, principally all pipe data is set by the program or updated depending on the Program override of user-entered values option. Only if you want to enter pipe data deviating from the standard pipeline must the pipe data be considered.

In the displayed grid, the data can only be viewed. To edit the data, you can open an entry window by double clicking on the display grid.