Valve factors 2_Vap. Med. 89 entry window_Incline exponent

Incline exponent

Enter the incline exponent for the acoustic efficiency for this operational case here.

During calculation of the valve, incline exponent is determined for a comparable SAMSON valve by the program and updated for the valve factors according to the setting of the Program override of user-entered values option.

see also:

5.5 G1 and G2 constants

4.3.5 VDMA 24422 (1989) for gases and vapors

4.3.9 SAMSON standard method with gases/vapors