[program]
fileformat_version=3.5
program_version=3.22
language=de
error=0
valve_cal=0
actuator_cal=0
[preferences]
database=Frei
calc_std=SAMSON
safety_f=1,1
unit_std=SI
[header]
item_no=
tag_no=
med_index=0
medium=Wasser
state=flüssig
state_index=0
valvet_index=0
actuatort_index=0
range_index=-1
[process]
q_ui=0
p1_ui=0
p2_ui=0
t1_ui=0
q_1=
p1_1=
p2_1=
t1_1=
q_2=
p1_2=
p2_2=
t1_2=
q_3=
p1_3=
p2_3=
t1_3=
[medium]
rho_ui=0
pv_ui=0
pc_ui=0
ny_ui=1
rho_1=
rho_2=
rho_3=
pv_1=
pv_2=
pv_3=
pc_1=
pc_2=
pc_3=
ny_1=
ny_2=
ny_3=
meddadbact_1=0
meddadbact_2=0
meddadbact_3=0
[flashing]
rhoxd2_ui=0
xd2_1=0
rhoxd2_1=0
xd2_2=0
rhoxd2_2=0
xd2_3=0
rhoxd2_3=0
[valve_1]
dn_ui=0
pn_ui=0
kvs_ui=0
travel_ui=0
sb_ui=0
series=
type=
dn=
pn=
bodymat=
noisred=
kvs=
charact=
fdirection=
travel=
sb=
series_v=
type_v=
dn_v=
pn_v=
bodymat_v=
noisred_v=
kvs_v=
charact_v=
fdirection_v=
[valve_2]
kd_ui=0
sd=
packing=
sealing=
balanced=
leakage=
bonnet=
packing_v=
sealing_v=
balanced_v=
leakage_v=
bonnet_v=
f1=0
f2=0
f3=0
[pipe]
dn1_ui=0
dn2_ui=0
cr_ui=0
rhor_ui=0
di_ui=0
ws_ui=0
isolation=
type=
dn1=
dn2=
cr=
rhor=
di=
s=
isolation_v=0
type_v=0
dn1_v=
dn2_v=
[actuator]
p1max_ui=0
p2min_ui=0
t1max_ui=0
diapha_ui=0
benchra_ui=0
supply_ui=0
p1max=
p2min=
t1max=
type=
failsafe=
diapha=
benchra=
supply=
type_v=
failsafe_v=
benchras_v=0
benchrae_v=0
[results_1]
kv_ui=0
dnreq_ui=0
w_ui=0
kv_1=
dnreq_1=
w_1=
spl_1=
flow_1=
kv_2=
dnreq_2=
w_2=
spl_2=
flow_2=
kv_3=
dnreq_3=
w_3=
spl_3=
flow_3=
kv_1_v=0
dnreq_1_v=0
flow_1_v=0
kv_2_v=0
dnreq_2_v=0
flow_2_v=0
kv_3_v=0
dnreq_3_v=0
flow_3_v=0
[results_2]
reltrav_1=
x_1=
fl_1=
kc_1=
fd_1=
reltrav_2=
x_2=
fl_2=
kc_2=
fd_2=
reltrav_3=
x_3=
fl_3=
kc_3=
fd_3=
[results_3]
zy_1=
f1_1=
f2_1=
dlf_1=
zy_2=
f1_2=
f2_2=
dlf_2=
zy_3=
f1_3=
f2_3=
dlf_3=
[results_4]
freq_wo=
freq_w=
fmax=
dpmax=
ps0req=
dps=
fa=
si_close=
frictionf=
si_open=
[p_header]
offer=
project=
customer=
enteredby=
[p_borders]
top_ui=0
left_ui=0
top=1,2
left=2
[limits]
maxw_ui=0
maxsdp=85
maxw=5
c_med_1=0
c_med_2=0
c_med_3=0
[sdp_printout]
fp_1=0
fr_1=0
rev_1=0
uvc_mavc_1=0
etaa_1=0
regimet_1=0
peakf_1=0
x_1=0
slpi89_1=0
slpa1m89_1=0
sdpadin_1=0
slpidin_1=0
slpa1mdin_1=0
yexp_1=0
fp_2=0
fr_2=0
rev_2=0
uvc_mavc_2=0
etaa_2=0
regimet_2=0
peakf_2=0
x_2=0
slpi89_2=0
slpa1m89_2=0
sdpadin_2=0
slpidin_2=0
slpa1mdin_2=0
yexp_2=0
fp_3=0
fr_3=0
rev_3=0
uvc_mavc_3=0
etaa_3=0
regimet_3=0
peakf_3=0
x_3=0
slpi89_3=0
slpa1m89_3=0
sdpadin_3=0
slpidin_3=0
slpa1mdin_3=0
yexp_3=0
lwi31_1=0
lwi31_2=0
lwi31_3=0
lwi63_1=0
lwi63_2=0
lwi61_3=0
lwi125_1=0
lwi125_2=0
lwi125_3=0
lwi250_1=0
lwi250_2=0
lwi250_3=0
lwi500_1=0
lwi500_2=0
lwi500_3=0
lwi1000_1=0
lwi1000_2=0
lwi1000_3=0
lwi2000_1=0
lwi2000_2=0
lwi2000_3=0
lwi4000_1=0
lwi4000_2=0
lwi4000_3=0
lwi8000_1=0
lwi8000_2=0
lwi8000_3=0
lwi16000_1=0
lwi16000_2=0
lwi16000_3=0
lwa31_1=0
lwa31_2=0
lwa31_3=0
lwa63_1=0
lwa63_2=0
lwa61_3=0
lwa125_1=0
lwa125_2=0
lwa125_3=0
lwa250_1=0
lwa250_2=0
lwa250_3=0
lwa500_1=0
lwa500_2=0
lwa500_3=0
lwa1000_1=0
lwa1000_2=0
lwa1000_3=0
lwa2000_1=0
lwa2000_2=0
lwa2000_3=0
lwa4000_1=0
lwa4000_2=0
lwa4000_3=0
lwa8000_1=0
lwa8000_2=0
lwa8000_3=0
lwa16000_1=0
lwa16000_2=0
lwa16000_3=0
