Position_Safety factor

Safety factor

This menu item opens a window in which you can edit the safety factor for determination of the Kvs value from the maximum possible required Kv value.

If, for example, a Kv value of 20 is required and the safety factor is 1.1 (10%), a Kvs value greater than or equal to 22 is sought.

The safety factor must be between 1 and 10.

In addition, the current safety factor for the Kvs value is displayed in the status bar and can be changed by double clicking on the display.

The setting always relates only to the active item.