Valve data 2 entry window_Pressure relief

Pressure relief

Select the pressure relief system or its sealing here.

For the selection "none", "graphite" and "PTFE", an appropriate friction coefficient is suggested and set dependent on the Program override of user-entered values option of the valve and actuator data group.

"None" is always set during the calculation of the valve if no indication has yet been made. Only one pressure relief system is selected during calculation of the actuator if no satisfactory actuator could be found without a pressure relief system.