Entry window_Valve inlet medium pressure

Medium pressure at valve inlet

Enter the pressure of the medium at the valve inlet here.

If one of the standard media (water, steam or air) is selected, a new calculation of the medium data will be carried out when this entry is changed depending on the Program override of user-entered values option for the medium data group in the Preferences menu.

For vaporous media there is a check to see whether the inlet temperature is greater than or equal to the saturated steam temperature. If a temperature has not yet been entered, it will be set equal to the saturated steam temperature.