Liquid media valve factor 1_ Pressure recovery

Pressure recovery

Enter the pressure recovery factor for this operational case here.

During calculation of the valve, the pressure recovery factor is determined for a comparable SAMSON valve by the program and updated for the valve factors according to the setting of the Program override of user-entered values option.

see also:

5.1 Fl-value and xT-value

3.2.6 Flow characteristics

3.2.2 Flow limitation