Cannot find satisfactory signal pressure range.

This message appears when the program does not find a signal pressure range in the database during calculation of a SAMSON actuator type for the combination of the selected nominal travel of the valve (Valve data part 1) and the selected actuator type and the selected diaphragm area.

In this case, further calculation is carried out as for a non-SAMSON type (see Calculate actuator).