Valve data 1 entry window_Nominal pressure level_1

Nominal pressure level

Enter the nominal pressure level of the valve here. The general nominal size series is offered in the list. There is no differentiation according to product line and type.

During calculation, the nominal size is selected by the program and updated for the valve and actuator data according to the setting of the Program override of user-entered values option. Therefore, the program always selects minimum PN 40.