Actuator data entry window_Diaphragm area

Diaphragm area

Enter the diaphragm area of the actuator here.

Which areas are included in the selection list is determined by the selected actuator type. Therefore, no areas are offered for non-SAMSON types.

During the calculation of the actuator, the appropriate diaphragm area for the SAMSON type is selected by the program and updated for the pipe data according to the setting of the Program override of user-entered values option.