Valve factors 2 liquid media 1989_Incline exponent

Incline exponent

Enter the incline exponent for the acoustic efficiency for this operational case here.

During calculation of the valve, the incline exponent is determined for a comparable SAMSON valve by the program and updated for the valve factors according to the setting of the Program override of user-entered values option.

see also:

5.6 F1 and F2 constants

4.3.7 VDMA 24422 (1989) or DIN IEC 534 Part 8-4 for liquids

4.3.10 SAMSON standard method with liquids