Valve factors 1_Entry window

Valve factors part 1 for liquid media entry window

Two results of the valve calculation are displayed in this window, and you can edit valve factors for all three operational cases.

Pressing the "Enter" key accesses the next entry field of the operational case being processed. This entry sequence will also guide users from the last entry field for the valve factors part 1 to the first entry field of the valve factors part 2 of the next operational case.

To exit the entry window, either click the "OK" button in the entry window, press the "Esc" key, or click your mouse on a point outside the entry window.

With valve types Regul. flanged, Regul. threaded, V2001 and HVAC, HVAC-threaded, the program indicates the rangeability (RNG) in place of the relative travel (rel. travel [%]).