valve factor 1_ Travel

Relative travel/safety factor

Depending on the selected valve type, either the relative travel (for globe, angle and three-way valves) or the safety factor (Kvs/Kv, for Regul. flanged/threaded, V2002 and HVAC, HVAC-threaded) calculated for this operational case is displayed here. The selected characteristic is included by the calculation of the relative travel.

Since the travel is only a result, this field cannot be edited.