Valve factors 1

Valve factors part 1

Valve factors and two results of the valve calculation are summarized in this entry page.

Various data is displayed depending on the aggregate state of the medium.

All data is indicated for all three operational cases (minimum, maximum and standard). The data is only displayed in the display grid. You can open an entry window for editing the data by double clicking on the display grid.

For valve types Regul. flanged/threaded, V2001 and HVAC, HVAC-threaded, the rangeability (RNG) is indicated in place of the relative travel (rel. travel [%]).

Valve factors part 1 for liquid media

Valve factors part 2 for vaporous and gaseous media