Process data check

It is checked whether the entered process data are plausible, i.e. whether they form a "reasonable" characteristic. For a real pump and plant characteristic, the operating case with minimum flow rate is associated with the maximum differential pressure, i.e. the maximum input pressure and the minimum output pressure. Correspondingly, the operating case with maximum flow rate is associated with the minimum differential pressure, i.e. the minimum input pressure and the maximum output pressure. This order of values is checked prior to calculation. If the order does not meet the above criteria, a message is displayed. The values for the flow rate can be brought into the right order (the pressures p1 and p2 remain unchanged).

The message can be deactivated...