Item Reverse calculation flow rate

Reverse calculation flow rate

Select this menu item to calculate the resulting flow rate for the entered process and medium data as well as for the currently active valve. The capacity for which the flow rate is calculated must be indicated by the Safety factor for the Kvs value.

For instance, if you enter a safety factor of 1.0, the program calculates which flow rate would result for the respective operating case at 100% travel. A safety factor of 2 would result in 50% capacity.