Valve factors 2 liquid media 1989_Level exponent

Level exponent

Enter the level exponent for the acoustic efficiency for this operational case here.

During calculation of the valve, the level exponent is determined by the program for a comparable SAMSON valve and updated for the valve factors according to the setting of the Program override of user-entered values option.

see also:

5.6 F1 and F2 constants

4.3.7 VDMA 24422 (1989) or DIN IEC 534 Part 8-4 for liquids

4.3.10 SAMSON standard method with liquids