Valve data 2 entry window_Leakage class

Leakage class

Enter the leakage class of the valve here.

During calculation, the leakage class is determined by the program according to the selected sealing edge and pressure relief system and updated for the valve and actuator data according to the setting of the Program override of user-entered values option.

Important: The specification of the leakage class is a pure outlet for the calculation. Selecting a particular leakage class before calculation therefore does not imply that it will be achieved by a corresponding sealing edge and pressure relief system.